**Supertrack KanLink Release Notes**

**Release KanLink A1 : TR**

Previous versions were incomplete

* **A1** Includes Clean side Client task and Std.Kanlink has been modified to be max number of Kanlink machines, not number – 1
* **A2** All tasks combined into 1 driver and a config task.
* **A3** New release of KGFramework – KGFrameworkshare required declaration updates.

Modified Client driver code.

* **A4** Added 2 standard states to Server and Client Driver.
* **A5** Added Server and client for Batch Info. (OverView)
* **A6**
* **A7** Add program and category number transfer option **DO NOT USE….**
* **A8.** Fixed Bugs in A7 with batch ID transfers..
* **A9** Removed global declaration of n
* **A10** Add cmdOpt to IP config to allow for multiple connections in 1 IP.
* **A11 –**
* **A12 –** correct code when checking for valid cat in driver
* **A13 –** Add Batch received to kanlink client interface.
* **A14 –** Add X20CP1586 to KG framework
* **A15 –** Add batching control to server (See additional Discharger example code)